\documentclass[letterpaper, 12pt, twoside]{article}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%

% Items to perhaps set up for each document

\newcommand{\mydate}{\textsf{April 17, 2003}}
\newcommand{\mylecture}{\textsf{Using the AIC10 EVM on the C5510 DSK}}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%

%********
\def\draftversion{Y}                % Y for draft, N for final version
%********

\include{../../NoteSetup}

\begin{document}

%\vspace{\baselineskip}

\begin{center}
\textbf{\Large \mylecture}
\end{center}

The AIC10 EVM uses McBSP port 0 and generates the framesync and clock signals.

Master and secondary each generate frame sync pulses.  Bit 0 of received sample
values use bit 0 to distinguish between units.

Bits are shifted out MSB first to LSB.  Same as with the AIC23.

Sample bits on negative going clock edges.  Opposite as with the AIC23.

\end{document}
